<?xml version="1.0" encoding="utf-8"?>
<JingJiBiao BiaoDuanNO="20260901001" Xmmc="“双百”专项行动—丁家村丁家庄人居环境整治工程" Bdmc="“双百”专项行动—丁家村丁家庄人居环境整治工程" HtLx="1" Jsfs="1" Version="4.0">
  <ZhaoBiaoXx Zbr="江苏省常州市新北区薛家镇丁家村村民委员会" ZbrDb="王云虎" BzTime="2026-08-31" Bzr="王鸿行" Shr="王鸿行" Bzdw="宏信天德工程顾问有限公司" BzdwDb="戴尚鹏">
    <ZhaoBiaoZsm xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:nil="true" />
    <GclQdJsgz>[encoded data, 183156 characters]</GclQdJsgz>
  </ZhaoBiaoXx>
  <Dxgcxx Dxgcbh="001" Dxgcmc="“双百”专项行动—丁家村丁家庄人居环境整治工程" QdxmHj="0" CsxmHj="0" AqscHj="0" QtxmHj="0" ZljeHj="0" ZygczgjHj="0" JrgHj="0" ZcbfwfHj="0" HtydqtxmHj="0" ZzsHj="0" Je="0">
    <Dwgcxx Dwgcbh="1" Dwgcmc="建筑工程" Zylb="1" SoftName="江苏国泰新点软件有限公司" SoftNum="E4E95290F428F9C746EF6C571E3FC20F9D390E78F56A798B15875A361C3A4337" DogNum="9733bf01000702019dc30006003c003d" MachineKey="3D889780543CF2AB12783945A792088C91F52798C4DAF50163FA09192FB72839">
  <Dwhz>
    <DwhzMx Xh="1" Mc="分部分项工程" Je="0" Fyxlb="1" />
    <DwhzMx Xh="2" Mc="措施项目" Je="0" Fyxlb="2" />
    <DwhzMx Xh="2.1" Mc="    其中：安全生产" Je="0" Fyxlb="2.1" />
    <DwhzMx Xh="3" Mc="其他项目" Je="0" Fyxlb="3" />
    <DwhzMx Xh="3.1" Mc="    其中：暂列金额" Je="0" Fyxlb="3.1" />
    <DwhzMx Xh="3.2" Mc="    其中：专业工程暂估价" Je="0" Fyxlb="3.2" />
    <DwhzMx Xh="3.3" Mc="    其中：计日工" Je="0" Fyxlb="3.3" />
    <DwhzMx Xh="3.4" Mc="    其中：总承包服务费" Je="0" Fyxlb="3.4" />
    <DwhzMx Xh="3.5" Mc="    其中：合同中约定的其他项目" Je="0" Fyxlb="3.5" />
    <DwhzMx Xh="4" Mc="增值税" Je="0" Fyxlb="4" />
    <DwhzMx Xh="5" Mc="工程造价" Je="0" Fyxlb="5" />
  </Dwhz>
  <Zzs>
    <ZzsMx Xh="1" Mc="增值税" Jsjc="分部分项工程+措施项目+其他项目-专业工程暂估价-除税甲供材料和甲供设备费" Qfjs="0" Fl="9" Je="0" />
  </Zzs>
  <Qdxm>
    <QdBt Xh="" Mc="建筑出新" Je="0" Zgj="0">
      <Qdmx Xh="1" Qdbm="011201001001" Mc="墙、柱面一般抹灰" Xmtz="1、原墙面装饰层铲除（含瓷砖、涂料、汰石子面层、原有抹灰等）至原有墙面，含铲除后的建筑垃圾外运，运距及垃圾处理费用自行考虑；&#xD;&#xA;2、聚合物水泥浆一道；&#xD;&#xA;3、5厚1:3水泥砂浆打底扫毛或划出纹道&#xD;&#xA;4、刷素水泥浆一道（内掺水重5%的建筑胶）&#xD;&#xA;5、6厚1:2.5水泥砂浆（内掺建筑胶）&#xD;&#xA;6、含脚手架或其他登高费用，投标单位自行考虑&#xD;&#xA;" Jsgz="按设计图示尺寸以面积计算。扣除墙裙、门窗洞口面积；不扣除单个面积≤0.3m2的孔洞面积，不扣除挂镜线、墙与构件交接处的面积；附墙柱、梁、垛、烟囱侧壁并入相应的墙面面积内；门窗洞口和孔洞的侧壁及顶面不增加面积" Dw="m2" Sl="1430" Zhdj="0" Zhhj="0" Rgf="0" Zcf="0" Fcf="0" Sbf="0" Clf="0" Jxf="0" Glf="0" Lr="0" Zgj="0" />
      <Qdmx Xh="2" Qdbm="011403001001" Mc="抹灰面油漆" Xmtz="外墙弹性涂料：批腻子两遍，外墙涂料三遍&#xD;&#xA;含脚手架或其他登高费用，投标单位自行考虑" Jsgz="按设计图示尺寸以面积计算" Dw="m2" Sl="1430" Zhdj="0" Zhhj="0" Rgf="0" Zcf="0" Fcf="0" Sbf="0" Clf="0" Jxf="0" Glf="0" Lr="0" Zgj="0" />
    </QdBt>
  </Qdxm>
  <Csxm>
    <CsxmBt Xh="" Mc="通用措施项目" Je="0" Bz="">
      <CsxmMx Xh="1" Bm="011601009001" Mc="安全生产" Gznr="" Dw="项" Je="0" Zb_CSSlF="0" Je_CSSlF="0" Zb_ZQYxF="0" Je_ZQYxF="0" Zb_HQCcF="0" Je_HQCcF="0" Qfjs="0" Jsjc="分部分项合计-除税工程设备费" Fl="3.8" Xmlb="1" Jjfs="2" Bz="" />
      <CsxmMx Xh="2" Bm="011601007001" Mc="文明施工" Gznr="" Dw="项" Je="0" Zb_CSSlF="0" Je_CSSlF="0" Zb_ZQYxF="0" Je_ZQYxF="0" Zb_HQCcF="0" Je_HQCcF="0" Qfjs="0" Jsjc="分部分项合计-除税工程设备费" Fl="0" Xmlb="0" Jjfs="2" Bz="" />
      <CsxmMx Xh="3" Bm="011601008001" Mc="环境保护" Gznr="" Dw="项" Je="0" Zb_CSSlF="0" Je_CSSlF="0" Zb_ZQYxF="0" Je_ZQYxF="0" Zb_HQCcF="0" Je_HQCcF="0" Qfjs="0" Jsjc="分部分项合计-除税工程设备费" Fl="0" Xmlb="0" Jjfs="2" Bz="" />
      <CsxmMx Xh="4" Bm="011601006001" Mc="临时设施" Gznr="" Dw="项" Je="0" Zb_CSSlF="0" Je_CSSlF="0" Zb_ZQYxF="0" Je_ZQYxF="0" Zb_HQCcF="0" Je_HQCcF="0" Qfjs="0" Jsjc="分部分项合计-除税工程设备费" Fl="0" Xmlb="0" Jjfs="2" Bz="" />
      <CsxmMx Xh="5" Bm="011601010001" Mc="冬雨季施工增加" Gznr="" Dw="项" Je="0" Zb_CSSlF="0" Je_CSSlF="0" Zb_ZQYxF="0" Je_ZQYxF="0" Zb_HQCcF="0" Je_HQCcF="0" Qfjs="0" Jsjc="分部分项合计-除税工程设备费" Fl="0" Xmlb="0" Jjfs="2" Bz="" />
      <CsxmMx Xh="6" Bm="011601011001" Mc="夜间施工增加" Gznr="" Dw="项" Je="0" Zb_CSSlF="0" Je_CSSlF="0" Zb_ZQYxF="0" Je_ZQYxF="0" Zb_HQCcF="0" Je_HQCcF="0" Qfjs="0" Jsjc="分部分项合计-除税工程设备费" Fl="0" Xmlb="0" Jjfs="2" Bz="" />
      <CsxmMx Xh="7" Bm="011601012001" Mc="特殊地区施工增加" Gznr="" Dw="项" Je="0" Zb_CSSlF="0" Je_CSSlF="0" Zb_ZQYxF="0" Je_ZQYxF="0" Zb_HQCcF="0" Je_HQCcF="0" Qfjs="0" Jsjc="分部分项合计-除税工程设备费" Fl="0" Xmlb="0" Jjfs="2" Bz="" />
      <CsxmMx Xh="8" Bm="011601013001" Mc="二次搬运" Gznr="" Dw="项" Je="0" Zb_CSSlF="0" Je_CSSlF="0" Zb_ZQYxF="0" Je_ZQYxF="0" Zb_HQCcF="0" Je_HQCcF="0" Qfjs="0" Jsjc="分部分项合计-除税工程设备费" Fl="0" Xmlb="0" Jjfs="2" Bz="" />
      <CsxmMx Xh="9" Bm="011601014001" Mc="已完工程及设备保护" Gznr="" Dw="项" Je="0" Zb_CSSlF="0" Je_CSSlF="0" Zb_ZQYxF="0" Je_ZQYxF="0" Zb_HQCcF="0" Je_HQCcF="0" Qfjs="0" Jsjc="分部分项合计-除税工程设备费" Fl="0" Xmlb="0" Jjfs="2" Bz="" />
      <CsxmMx Xh="10" Bm="011601015001" Mc="既有建(构)筑物、设施保护" Gznr="" Dw="项" Je="0" Zb_CSSlF="0" Je_CSSlF="0" Zb_ZQYxF="0" Je_ZQYxF="0" Zb_HQCcF="0" Je_HQCcF="0" Qfjs="0" Jsjc="分部分项合计-除税工程设备费" Fl="0" Xmlb="0" Jjfs="2" Bz="" />
      <CsxmMx Xh="11" Bm="011601016001" Mc="按质论价" Gznr="" Dw="项" Je="0" Zb_CSSlF="0" Je_CSSlF="0" Zb_ZQYxF="0" Je_ZQYxF="0" Zb_HQCcF="0" Je_HQCcF="0" Qfjs="0" Jsjc="分部分项合计-除税工程设备费" Fl="0" Xmlb="2" Jjfs="2" Bz="" />
      <CsxmMx Xh="12" Bm="011601017001" Mc="建筑工人实名制" Gznr="" Dw="项" Je="0" Zb_CSSlF="0" Je_CSSlF="0" Zb_ZQYxF="0" Je_ZQYxF="0" Zb_HQCcF="0" Je_HQCcF="0" Qfjs="0" Jsjc="分部分项合计-除税工程设备费" Fl="0" Xmlb="0" Jjfs="2" Bz="" />
      <CsxmMx Xh="13" Bm="011601018001" Mc="特殊施工降效" Gznr="" Dw="项" Je="0" Zb_CSSlF="0" Je_CSSlF="0" Zb_ZQYxF="0" Je_ZQYxF="0" Zb_HQCcF="0" Je_HQCcF="0" Qfjs="0" Jsjc="分部分项合计-除税工程设备费" Fl="0" Xmlb="0" Jjfs="2" Bz="" />
      <CsxmMx Xh="14" Bm="011601019001" Mc="协管" Gznr="" Dw="项" Je="0" Zb_CSSlF="0" Je_CSSlF="0" Zb_ZQYxF="0" Je_ZQYxF="0" Zb_HQCcF="0" Je_HQCcF="0" Qfjs="0" Jsjc="分部分项合计-除税工程设备费" Fl="0" Xmlb="0" Jjfs="2" Bz="" />
    </CsxmBt>
    <CsxmBt Xh="" Mc="专业措施项目" Je="0" Bz="" />
  </Csxm>
  <Qtxm>
    <QtxmMx Xh="1" Mc="暂列金额" Je="0" Bz="详见本标准表E.4.2" Xmlb="1" />
    <QtxmMx Xh="2" Mc="专业工程暂估价" Je="0" Bz="详见本标准表E.4.3" Xmlb="2" />
    <QtxmMx Xh="3" Mc="计日工" Je="0" Bz="详见本标准表E.4.4" Xmlb="3" />
    <QtxmMx Xh="4" Mc="总承包服务费" Je="0" Bz="详见本标准表E.4.5" Xmlb="4" />
    <QtxmMx Xh="5" Mc="合同中约定的其他项目" Je="0" Bz="" Xmlb="5" />
  </Qtxm>
  <Zlje>
    <ZljeBt Xh="1" Mc="合同价格调整暂列金额" Je="0" Xmlb="1" />
    <ZljeBt Xh="2" Mc="未确定工程暂列金额" Je="0" Xmlb="2" />
    <ZljeBt Xh="3" Mc="未确定服务暂列金额" Je="0" Xmlb="3" />
    <ZljeBt Xh="4" Mc="未确定其他暂列金额" Je="0" Xmlb="4" />
  </Zlje>
  <Zygczgj />
  <Jrg>
    <JrgBt Bh="一" Mc="人工" Je="0" Xmlb="1" />
    <JrgBt Bh="二" Mc="材料" Je="0" Xmlb="2" />
    <JrgBt Bh="三" Mc="施工机具" Je="0" Xmlb="3" />
  </Jrg>
  <Zcbfwf>
    <ZcbfwfBt Xh="1" Mc="发包人提供材料" Je="0" Xmlb="1" />
    <ZcbfwfBt Xh="2" Mc="专业分包工程" Je="0" Xmlb="2" />
    <ZcbfwfBt Xh="3" Mc="直接发包的专业工程" Je="0" Xmlb="3" />
  </Zcbfwf>
  <Clzg />
  <Fbrgycl />
  <CbrgyclCef />
  <Rcjhz />
</Dwgcxx>
    <Dwgcxx Dwgcbh="2" Dwgcmc="景观工程" Zylb="5" SoftName="江苏国泰新点软件有限公司" SoftNum="6344DB4A1DAF71B242E9E7F73EC8DA909D390E78F56A798B15875A361C3A4337" DogNum="9733bf01000702019dc30006003c003d" MachineKey="891A361C86623C4E977A14FED861D2DB8A23C91DE32C07E1AF9DB651D897C3E2">
  <Dwhz>
    <DwhzMx Xh="1" Mc="分部分项工程" Je="0" Fyxlb="1" />
    <DwhzMx Xh="2" Mc="措施项目" Je="0" Fyxlb="2" />
    <DwhzMx Xh="2.1" Mc="    其中：安全生产" Je="0" Fyxlb="2.1" />
    <DwhzMx Xh="3" Mc="其他项目" Je="0" Fyxlb="3" />
    <DwhzMx Xh="3.1" Mc="    其中：暂列金额" Je="0" Fyxlb="3.1" />
    <DwhzMx Xh="3.2" Mc="    其中：专业工程暂估价" Je="0" Fyxlb="3.2" />
    <DwhzMx Xh="3.3" Mc="    其中：计日工" Je="0" Fyxlb="3.3" />
    <DwhzMx Xh="3.4" Mc="    其中：总承包服务费" Je="0" Fyxlb="3.4" />
    <DwhzMx Xh="3.5" Mc="    其中：合同中约定的其他项目" Je="0" Fyxlb="3.5" />
    <DwhzMx Xh="4" Mc="增值税" Je="0" Fyxlb="4" />
    <DwhzMx Xh="5" Mc="工程造价" Je="0" Fyxlb="5" />
  </Dwhz>
  <Zzs>
    <ZzsMx Xh="1" Mc="增值税" Jsjc="分部分项工程+措施项目+其他项目-专业工程暂估价-除税甲供材料和甲供设备费" Qfjs="0" Fl="9" Je="0" />
  </Zzs>
  <Qdxm>
    <QdBt Xh="" Mc="一、村里其他" Je="0" Zgj="0">
      <QdBt Xh="" Mc="1、彩绘" Je="0" Zgj="0">
        <Qdmx Xh="1" Qdbm="011404001001" Mc="墙面喷刷涂料" Xmtz="建筑外立面彩绘;滚涂抗碱封闭底漆;喷涂3mm丙烯彩绘;喷涂环保清漆一层&#xD;&#xA;含脚手架或其他登高费用，投标单位自行考虑" Jsgz="按设计图示尺寸以展开面积计算。洞口侧壁面积并入相应喷刷部位中计算" Dw="m2" Sl="50" Zhdj="0" Zhhj="0" Rgf="0" Zcf="0" Fcf="0" Sbf="0" Clf="0" Jxf="0" Glf="0" Lr="0" Zgj="0" />
      </QdBt>
      <QdBt Xh="" Mc="2、篱笆" Je="0" Zgj="0">
        <Qdmx Xh="2" Qdbm="050307007004" Mc="围栏" Xmtz="成品不锈钢仿竹篱笆&#xD;&#xA;地面以上350mm高，含C20素砼基础&#xD;&#xA;立柱φ51*0.5，横管φ25*0.4，斜管φ19*0.3，烤漆" Jsgz="按设计图示围栏尺寸以中心线长度计算" Dw="m" Sl="150" Zhdj="0" Zhhj="0" Rgf="0" Zcf="0" Fcf="0" Sbf="0" Clf="0" Jxf="0" Glf="0" Lr="0" Zgj="0" />
        <Qdmx Xh="3" Qdbm="050307007005" Mc="围栏" Xmtz="水泥仿木栅栏&#xD;&#xA;φ150，插入地下200深&#xD;&#xA;标准段高低五连排（露出地面150mm高~300高）" Jsgz="按设计图示围栏尺寸以中心线长度计算" Dw="m" Sl="170.45" Zhdj="0" Zhhj="0" Rgf="0" Zcf="0" Fcf="0" Sbf="0" Clf="0" Jxf="0" Glf="0" Lr="0" Zgj="0" />
      </QdBt>
      <QdBt Xh="" Mc="3、水泥栅栏" Je="0" Zgj="0">
        <Qdmx Xh="4" Qdbm="050307007003" Mc="围栏" Xmtz="水泥仿木栅栏三;&#xD;&#xA;水泥竹节五连排桩，φ100C20预制砼柱，仿竹节;露出地面270~320，含立柱基础及垫层;" Jsgz="按设计图示围栏尺寸以中心线长度计算" Dw="m" Sl="800" Zhdj="0" Zhhj="0" Rgf="0" Zcf="0" Fcf="0" Sbf="0" Clf="0" Jxf="0" Glf="0" Lr="0" Zgj="0" />
      </QdBt>
    </QdBt>
    <QdBt Xh="" Mc="二、村西节点" Je="0" Zgj="0">
      <QdBt Xh="" Mc="1、入口景墙" Je="0" Zgj="0">
        <Qdmx Xh="5" Qdbm="040101002002" Mc="挖沟槽土方" Xmtz="挖土类型、土壤类别、挖土深度综合考虑，含场内运输" Jsgz="按设计图示基础尺寸(含垫层)底面积另加工作面面积乘以开挖深度，以体积计算" Dw="m3" Sl="15.91" Zhdj="0" Zhhj="0" Rgf="0" Zcf="0" Fcf="0" Sbf="0" Clf="0" Jxf="0" Glf="0" Lr="0" Zgj="0" />
        <Qdmx Xh="6" Qdbm="040103001002" Mc="沟槽、基坑回填方" Xmtz="沟槽土方回填，满足图纸设计的标高和压实度要求;" Jsgz="按挖方清单项目工程量加原地面标高至设计要求标高间的体积，减基础、构筑物等埋入体积计算" Dw="m3" Sl="8.9" Zhdj="0" Zhhj="0" Rgf="0" Zcf="0" Fcf="0" Sbf="0" Clf="0" Jxf="0" Glf="0" Lr="0" Zgj="0" />
        <Qdmx Xh="7" Qdbm="040103003002" Mc="余方弃置" Xmtz="余土外运;运距、堆场及处置等费用由投标单位综合考虑;" Jsgz="按挖方清单项目工程量减回填利用方体积(正数)计算" Dw="m3" Sl="7.01" Zhdj="0" Zhhj="0" Rgf="0" Zcf="0" Fcf="0" Sbf="0" Clf="0" Jxf="0" Glf="0" Lr="0" Zgj="0" />
        <Qdmx Xh="8" Qdbm="010501001001" Mc="基础垫层" Xmtz="100厚C20混凝土垫层" Jsgz="按设计图示尺寸以体积计算。不扣除伸入垫层的桩头所占体积" Dw="m3" Sl="1.91" Zhdj="0" Zhhj="0" Rgf="0" Zcf="0" Fcf="0" Sbf="0" Clf="0" Jxf="0" Glf="0" Lr="0" Zgj="0" />
        <Qdmx Xh="9" Qdbm="010505001001" Mc="垫层模板" Xmtz="景墙垫层木模" Jsgz="按模板与现浇混凝土垫层的接触面积计算" Dw="m2" Sl="2.27" Zhdj="0" Zhhj="0" Rgf="0" Zcf="0" Fcf="0" Sbf="0" Clf="0" Jxf="0" Glf="0" Lr="0" Zgj="0" />
        <Qdmx Xh="10" Qdbm="050307009002" Mc="景墙" Xmtz="M7.5水泥砂浆砌100~300大小黄色自然石块（不低于MU30）表面要求选择平整且对缝的石块，缝宽小于8mm，不勾缝" Jsgz="按设计图示尺寸以体积计算" Dw="m3" Sl="12.62" Zhdj="0" Zhhj="0" Rgf="0" Zcf="0" Fcf="0" Sbf="0" Clf="0" Jxf="0" Glf="0" Lr="0" Zgj="0" />
        <Qdmx Xh="11" Qdbm="050307020001" Mc="其他景观小摆设" Xmtz="水泥砂浆浮雕卡通形象，厚度30-50，彩绘。详见图纸" Jsgz="按设计图示数量计算" Dw="个" Sl="5" Zhdj="0" Zhhj="0" Rgf="0" Zcf="0" Fcf="0" Sbf="0" Clf="0" Jxf="0" Glf="0" Lr="0" Zgj="0" />
        <Qdmx Xh="12" Qdbm="050304003001" Mc="金属花架柱、梁" Xmtz="成品铁艺门洞 25方管 2400高 2000宽 400深&#xD;&#xA;详见图纸要求" Jsgz="按设计图示尺寸以质量计算" Dw="个" Sl="1" Zhdj="0" Zhhj="0" Rgf="0" Zcf="0" Fcf="0" Sbf="0" Clf="0" Jxf="0" Glf="0" Lr="0" Zgj="0" />
        <Qdmx Xh="13" Qdbm="011508001001" Mc="美术字" Xmtz="“丁家菜园” &#xD;&#xA;不锈钢立体字，表面烤漆，彩色，高度600，含基础及预埋件" Jsgz="按设计图示数量计算" Dw="个" Sl="4" Zhdj="0" Zhhj="0" Rgf="0" Zcf="0" Fcf="0" Sbf="0" Clf="0" Jxf="0" Glf="0" Lr="0" Zgj="0" />
        <Qdmx Xh="14" Qdbm="050307008001" Mc="标志牌" Xmtz="玻璃钢卡通立体形象&#xD;&#xA;规格、颜色、做法详见图纸要求" Jsgz="按设计图示数量计算" Dw="个" Sl="1" Zhdj="0" Zhhj="0" Rgf="0" Zcf="0" Fcf="0" Sbf="0" Clf="0" Jxf="0" Glf="0" Lr="0" Zgj="0" />
      </QdBt>
      <QdBt Xh="" Mc="2、彩绘" Je="0" Zgj="0">
        <Qdmx Xh="15" Qdbm="011404001002" Mc="墙面喷刷涂料" Xmtz="建筑外立面彩绘;滚涂抗碱封闭底漆;喷涂3mm丙烯彩绘;喷涂环保清漆一层" Jsgz="按设计图示尺寸以展开面积计算。洞口侧壁面积并入相应喷刷部位中计算" Dw="m2" Sl="200" Zhdj="0" Zhhj="0" Rgf="0" Zcf="0" Fcf="0" Sbf="0" Clf="0" Jxf="0" Glf="0" Lr="0" Zgj="0" />
      </QdBt>
      <QdBt Xh="" Mc="4、篱笆" Je="0" Zgj="0">
        <Qdmx Xh="16" Qdbm="050307007006" Mc="围栏" Xmtz="成品不锈钢仿竹篱笆&#xD;&#xA;地面以上350mm高，含C20素砼基础&#xD;&#xA;立柱φ51*0.5，横管φ25*0.4，斜管φ19*0.3，烤漆" Jsgz="按设计图示围栏尺寸以中心线长度计算" Dw="m" Sl="40" Zhdj="0" Zhhj="0" Rgf="0" Zcf="0" Fcf="0" Sbf="0" Clf="0" Jxf="0" Glf="0" Lr="0" Zgj="0" />
        <Qdmx Xh="17" Qdbm="050307007007" Mc="围栏" Xmtz="水泥仿木栅栏&#xD;&#xA;φ150，插入地下200深&#xD;&#xA;标准段高低五连排（露出地面150mm高~300高）" Jsgz="按设计图示围栏尺寸以中心线长度计算" Dw="m" Sl="40" Zhdj="0" Zhhj="0" Rgf="0" Zcf="0" Fcf="0" Sbf="0" Clf="0" Jxf="0" Glf="0" Lr="0" Zgj="0" />
      </QdBt>
      <QdBt Xh="" Mc="5、驳岸梳理（清杂打桩）" Je="0" Zgj="0">
        <Qdmx Xh="18" Qdbm="050202002001" Mc="原木桩驳岸" Xmtz="φ120杉木桩单排密打 L=2000&#xD;&#xA;木桩采用带皮杉木" Jsgz="按设计图示数量计算" Dw="根" Sl="2001" Zhdj="0" Zhhj="0" Rgf="0" Zcf="0" Fcf="0" Sbf="0" Clf="0" Jxf="0" Glf="0" Lr="0" Zgj="0" />
      </QdBt>
      <QdBt Xh="" Mc="7、码头修复" Je="0" Zgj="0">
        <Qdmx Xh="19" Qdbm="040305004001" Mc="砖砌体" Xmtz="M5标准砖小型砌体​" Jsgz="按设计图示尺寸以体积计算" Dw="m3" Sl="0.3" Zhdj="0" Zhhj="0" Rgf="0" Zcf="0" Fcf="0" Sbf="0" Clf="0" Jxf="0" Glf="0" Lr="0" Zgj="0" />
        <Qdmx Xh="20" Qdbm="040304003001" Mc="预制混凝土板" Xmtz="码头更换预制板" Jsgz="按设计图示尺寸以面积计算" Dw="m2" Sl="1" Zhdj="0" Zhhj="0" Rgf="0" Zcf="0" Fcf="0" Sbf="0" Clf="0" Jxf="0" Glf="0" Lr="0" Zgj="0" />
      </QdBt>
      <QdBt Xh="" Mc="8、道路重做修复" Je="0" Zgj="0">
        <Qdmx Xh="21" Qdbm="041001001001" Mc="拆除路面" Xmtz="拆除砼路面、水稳,二灰碎石,各种障碍物，砖砌体，石砌体，侧平石，道板等，拆除物归堆，含废料外运，弃场及运距自行考虑" Jsgz="按拆除部位以面积乘以厚度以体积计算" Dw="m3" Sl="90" Zhdj="0" Zhhj="0" Rgf="0" Zcf="0" Fcf="0" Sbf="0" Clf="0" Jxf="0" Glf="0" Lr="0" Zgj="0" />
        <Qdmx Xh="22" Qdbm="050201001002" Mc="园路垫层" Xmtz="100厚级配碎石" Jsgz="按设计图示尺寸以面积计算，不包括路牙，不扣除单个面积0.5m2以内的孔洞" Dw="m2" Sl="300" Zhdj="0" Zhhj="0" Rgf="0" Zcf="0" Fcf="0" Sbf="0" Clf="0" Jxf="0" Glf="0" Lr="0" Zgj="0" />
        <Qdmx Xh="23" Qdbm="050201003002" Mc="园路面层" Xmtz="20cm厚C30水泥混凝土路面，含养生、切缝、灌缝、模板等所有工作内容" Jsgz="按设计图示尺寸以面积计算，不包括路牙，不扣除单个面积0.5m2以内的孔洞" Dw="m2" Sl="300" Zhdj="0" Zhhj="0" Rgf="0" Zcf="0" Fcf="0" Sbf="0" Clf="0" Jxf="0" Glf="0" Lr="0" Zgj="0" />
        <Qdmx Xh="24" Qdbm="050201003003" Mc="园路面层" Xmtz="修复路面厚度每增减1cm;实际修复路面厚度如有调整，按本条清单调整" Jsgz="按设计图示尺寸以面积计算，不包括路牙，不扣除单个面积0.5m2以内的孔洞" Dw="m2" Sl="300" Zhdj="0" Zhhj="0" Rgf="0" Zcf="0" Fcf="0" Sbf="0" Clf="0" Jxf="0" Glf="0" Lr="0" Zgj="0" />
      </QdBt>
      <QdBt Xh="" Mc="9、园路（0.4及0.8m宽）" Je="0" Zgj="0">
        <Qdmx Xh="25" Qdbm="050201001003" Mc="园路垫层" Xmtz="100厚碎石垫层，素土夯实" Jsgz="按设计图示尺寸以面积计算，不包括路牙，不扣除单个面积0.5m2以内的孔洞" Dw="m2" Sl="210" Zhdj="0" Zhhj="0" Rgf="0" Zcf="0" Fcf="0" Sbf="0" Clf="0" Jxf="0" Glf="0" Lr="0" Zgj="0" />
        <Qdmx Xh="26" Qdbm="050201003004" Mc="园路面层" Xmtz="0.8m宽步道&#xD;&#xA;浅灰色水泥砖（400*400*50）铺贴，红色水泥砖(100*200*50)走边" Jsgz="按设计图示尺寸以面积计算，不包括路牙，不扣除单个面积0.5m2以内的孔洞" Dw="m2" Sl="120" Zhdj="0" Zhhj="0" Rgf="0" Zcf="0" Fcf="0" Sbf="0" Clf="0" Jxf="0" Glf="0" Lr="0" Zgj="0" />
        <Qdmx Xh="27" Qdbm="050201003005" Mc="园路面层" Xmtz="0.4m宽步道&#xD;&#xA;浅灰色水泥砖（400*400*50）铺贴" Jsgz="按设计图示尺寸以面积计算，不包括路牙，不扣除单个面积0.5m2以内的孔洞" Dw="m2" Sl="40" Zhdj="0" Zhhj="0" Rgf="0" Zcf="0" Fcf="0" Sbf="0" Clf="0" Jxf="0" Glf="0" Lr="0" Zgj="0" />
      </QdBt>
      <QdBt Xh="" Mc="十、菜地水泥板" Je="0" Zgj="0">
        <Qdmx Xh="28" Qdbm="050201003008" Mc="园路面层" Xmtz="原地面整平压实&#xD;&#xA;铺设成品预制水泥板，外宽50cm，详见图纸做法，含转角，以中心线长度计量" Jsgz="按设计中心线长度" Dw="m" Sl="30" Zhdj="0" Zhhj="0" Rgf="0" Zcf="0" Fcf="0" Sbf="0" Clf="0" Jxf="0" Glf="0" Lr="0" Zgj="0" />
      </QdBt>
    </QdBt>
    <QdBt Xh="" Mc="三、中心河塘运动健身场地" Je="0" Zgj="0">
      <QdBt Xh="" Mc="1、彩绘" Je="0" Zgj="0">
        <Qdmx Xh="29" Qdbm="011404001003" Mc="墙面喷刷涂料" Xmtz="建筑外立面彩绘;滚涂抗碱封闭底漆;喷涂3mm丙烯彩绘;喷涂环保清漆一层" Jsgz="按设计图示尺寸以展开面积计算。洞口侧壁面积并入相应喷刷部位中计算" Dw="m2" Sl="80" Zhdj="0" Zhhj="0" Rgf="0" Zcf="0" Fcf="0" Sbf="0" Clf="0" Jxf="0" Glf="0" Lr="0" Zgj="0" />
      </QdBt>
      <QdBt Xh="" Mc="2、排水管" Je="0" Zgj="0">
        <Qdmx Xh="30" Qdbm="040101002003" Mc="挖沟槽土方" Xmtz="挖土类型、土壤类别、挖土深度综合考虑，含场内运输" Jsgz="按设计图示基础尺寸(含垫层)底面积另加工作面面积乘以开挖深度，以体积计算" Dw="m3" Sl="124.65" Zhdj="0" Zhhj="0" Rgf="0" Zcf="0" Fcf="0" Sbf="0" Clf="0" Jxf="0" Glf="0" Lr="0" Zgj="0" />
        <Qdmx Xh="31" Qdbm="040103001003" Mc="沟槽、基坑回填方" Xmtz="沟槽土方回填，满足图纸设计的标高和压实度要求;" Jsgz="按挖方清单项目工程量加原地面标高至设计要求标高间的体积，减基础、构筑物等埋入体积计算" Dw="m3" Sl="104.47" Zhdj="0" Zhhj="0" Rgf="0" Zcf="0" Fcf="0" Sbf="0" Clf="0" Jxf="0" Glf="0" Lr="0" Zgj="0" />
        <Qdmx Xh="32" Qdbm="040103003003" Mc="余方弃置" Xmtz="余土外运;运距、堆场及处置等费用由投标单位综合考虑;" Jsgz="按挖方清单项目工程量减回填利用方体积(正数)计算" Dw="m3" Sl="20.18" Zhdj="0" Zhhj="0" Rgf="0" Zcf="0" Fcf="0" Sbf="0" Clf="0" Jxf="0" Glf="0" Lr="0" Zgj="0" />
        <Qdmx Xh="33" Qdbm="040501001002" Mc="混凝土管" Xmtz="1.基础材质、形式及厚度：100厚C15砼&#xD;&#xA;2.管道规格、等级：钢筋砼承插二级管 dn500" Jsgz="按设计图示中心线长度计算，不扣除管道附属构筑物、管件及阀门等所占长度" Dw="m" Sl="40" Zhdj="0" Zhhj="0" Rgf="0" Zcf="0" Fcf="0" Sbf="0" Clf="0" Jxf="0" Glf="0" Lr="0" Zgj="0" />
        <Qdmx Xh="34" Qdbm="040501001003" Mc="混凝土管" Xmtz="1.基础材质、形式及厚度：100厚C15砼&#xD;&#xA;2.管道规格、等级：钢筋砼承插二级管 dn600" Jsgz="按设计图示中心线长度计算，不扣除管道附属构筑物、管件及阀门等所占长度" Dw="m" Sl="10" Zhdj="0" Zhhj="0" Rgf="0" Zcf="0" Fcf="0" Sbf="0" Clf="0" Jxf="0" Glf="0" Lr="0" Zgj="0" />
      </QdBt>
      <QdBt Xh="" Mc="4、篱笆" Je="0" Zgj="0">
        <Qdmx Xh="35" Qdbm="050307007008" Mc="围栏" Xmtz="成品不锈钢仿竹篱笆&#xD;&#xA;地面以上350mm高，含C20素砼基础&#xD;&#xA;立柱φ51*0.5，横管φ25*0.4，斜管φ19*0.3，烤漆" Jsgz="按设计图示围栏尺寸以中心线长度计算" Dw="m" Sl="30" Zhdj="0" Zhhj="0" Rgf="0" Zcf="0" Fcf="0" Sbf="0" Clf="0" Jxf="0" Glf="0" Lr="0" Zgj="0" />
        <Qdmx Xh="36" Qdbm="050307007009" Mc="围栏" Xmtz="水泥仿木栅栏&#xD;&#xA;φ150，插入地下200深&#xD;&#xA;标准段高低五连排（露出地面150mm高~300高）" Jsgz="按设计图示围栏尺寸以中心线长度计算" Dw="m" Sl="30" Zhdj="0" Zhhj="0" Rgf="0" Zcf="0" Fcf="0" Sbf="0" Clf="0" Jxf="0" Glf="0" Lr="0" Zgj="0" />
      </QdBt>
      <QdBt Xh="" Mc="5、驳岸梳理（清杂打桩）" Je="0" Zgj="0">
        <Qdmx Xh="37" Qdbm="050202002002" Mc="原木桩驳岸" Xmtz="φ120杉木桩单排密打 L=2000&#xD;&#xA;木桩采用带皮杉木" Jsgz="按设计图示数量计算" Dw="根" Sl="351" Zhdj="0" Zhhj="0" Rgf="0" Zcf="0" Fcf="0" Sbf="0" Clf="0" Jxf="0" Glf="0" Lr="0" Zgj="0" />
      </QdBt>
      <QdBt Xh="" Mc="6、码头修复" Je="0" Zgj="0">
        <Qdmx Xh="38" Qdbm="040305004002" Mc="砖砌体" Xmtz="M5标准砖小型砌体​" Jsgz="按设计图示尺寸以体积计算" Dw="m3" Sl="0.3" Zhdj="0" Zhhj="0" Rgf="0" Zcf="0" Fcf="0" Sbf="0" Clf="0" Jxf="0" Glf="0" Lr="0" Zgj="0" />
        <Qdmx Xh="39" Qdbm="040304003002" Mc="预制混凝土板" Xmtz="码头更换预制板" Jsgz="按设计图示尺寸以面积计算" Dw="m2" Sl="1" Zhdj="0" Zhhj="0" Rgf="0" Zcf="0" Fcf="0" Sbf="0" Clf="0" Jxf="0" Glf="0" Lr="0" Zgj="0" />
      </QdBt>
      <QdBt Xh="" Mc="8、砖斜插收边" Je="0" Zgj="0">
        <Qdmx Xh="40" Qdbm="050201011001" Mc="路牙" Xmtz="200*100*60青砖斜插入200*150C25砼基础&#xD;&#xA;详见图纸做法，单价含基础模板、土方等全部工作内容" Jsgz="按设计图示尺寸以中心线长度计算" Dw="m" Sl="40" Zhdj="0" Zhhj="0" Rgf="0" Zcf="0" Fcf="0" Sbf="0" Clf="0" Jxf="0" Glf="0" Lr="0" Zgj="0" />
      </QdBt>
      <QdBt Xh="" Mc="9、园路（0.4及0.8m宽）" Je="0" Zgj="0">
        <Qdmx Xh="41" Qdbm="050201001004" Mc="园路垫层" Xmtz="100厚碎石垫层，素土夯实" Jsgz="按设计图示尺寸以面积计算，不包括路牙，不扣除单个面积0.5m2以内的孔洞" Dw="m2" Sl="126" Zhdj="0" Zhhj="0" Rgf="0" Zcf="0" Fcf="0" Sbf="0" Clf="0" Jxf="0" Glf="0" Lr="0" Zgj="0" />
        <Qdmx Xh="42" Qdbm="050201003006" Mc="园路面层" Xmtz="0.8m宽步道&#xD;&#xA;浅灰色水泥砖（400*400*50）铺贴，红色水泥砖(100*200*50)走边" Jsgz="按设计图示尺寸以面积计算，不包括路牙，不扣除单个面积0.5m2以内的孔洞" Dw="m2" Sl="72" Zhdj="0" Zhhj="0" Rgf="0" Zcf="0" Fcf="0" Sbf="0" Clf="0" Jxf="0" Glf="0" Lr="0" Zgj="0" />
        <Qdmx Xh="43" Qdbm="050201003007" Mc="园路面层" Xmtz="0.4m宽步道&#xD;&#xA;浅灰色水泥砖（400*400*50）铺贴" Jsgz="按设计图示尺寸以面积计算，不包括路牙，不扣除单个面积0.5m2以内的孔洞" Dw="m2" Sl="24" Zhdj="0" Zhhj="0" Rgf="0" Zcf="0" Fcf="0" Sbf="0" Clf="0" Jxf="0" Glf="0" Lr="0" Zgj="0" />
      </QdBt>
      <QdBt Xh="" Mc="10、运动场地" Je="0" Zgj="0">
        <Qdmx Xh="44" Qdbm="040101001001" Mc="挖一般土方" Xmtz="场地挖方，含清表，土方类别综合考虑，含场内运输" Jsgz="按设计图示尺寸以体积计算" Dw="m3" Sl="84.67" Zhdj="0" Zhhj="0" Rgf="0" Zcf="0" Fcf="0" Sbf="0" Clf="0" Jxf="0" Glf="0" Lr="0" Zgj="0" />
        <Qdmx Xh="45" Qdbm="040101005001" Mc="挖淤泥、流砂" Xmtz="原有河塘淤泥挖除并外运，运距及弃置投标人自行考虑" Jsgz="按设计图示位置及范围以体积计算" Dw="m3" Sl="450" Zhdj="0" Zhhj="0" Rgf="0" Zcf="0" Fcf="0" Sbf="0" Clf="0" Jxf="0" Glf="0" Lr="0" Zgj="0" />
        <Qdmx Xh="46" Qdbm="040103002001" Mc="一般回填方" Xmtz="300厚毛渣石回填" Jsgz="按设计图示尺寸以体积计算" Dw="m3" Sl="90" Zhdj="0" Zhhj="0" Rgf="0" Zcf="0" Fcf="0" Sbf="0" Clf="0" Jxf="0" Glf="0" Lr="0" Zgj="0" />
        <Qdmx Xh="47" Qdbm="040103002002" Mc="一般回填方" Xmtz="建筑碎渣回填 分层压实每350一道 压实度≥93%" Jsgz="按设计图示尺寸以体积计算" Dw="m3" Sl="1110" Zhdj="0" Zhhj="0" Rgf="0" Zcf="0" Fcf="0" Sbf="0" Clf="0" Jxf="0" Glf="0" Lr="0" Zgj="0" />
        <Qdmx Xh="48" Qdbm="040101002004" Mc="挖沟槽土方" Xmtz="挖土类型、土壤类别、挖土深度综合考虑，含场内运输;" Jsgz="按设计图示基础尺寸(含垫层)底面积另加工作面面积乘以开挖深度，以体积计算" Dw="m3" Sl="22.9" Zhdj="0" Zhhj="0" Rgf="0" Zcf="0" Fcf="0" Sbf="0" Clf="0" Jxf="0" Glf="0" Lr="0" Zgj="0" />
        <Qdmx Xh="49" Qdbm="040103001004" Mc="沟槽、基坑回填方" Xmtz="沟槽土方回填，满足图纸设计的标高和压实度要求" Jsgz="按挖方清单项目工程量加原地面标高至设计要求标高间的体积，减基础、构筑物等埋入体积计算" Dw="m3" Sl="1.97" Zhdj="0" Zhhj="0" Rgf="0" Zcf="0" Fcf="0" Sbf="0" Clf="0" Jxf="0" Glf="0" Lr="0" Zgj="0" />
        <Qdmx Xh="50" Qdbm="040103003004" Mc="余方弃置" Xmtz="余土外运;运距、堆场及处置等费用由投标单位综合考虑" Jsgz="按挖方清单项目工程量减回填利用方体积(正数)计算" Dw="m3" Sl="105.6" Zhdj="0" Zhhj="0" Rgf="0" Zcf="0" Fcf="0" Sbf="0" Clf="0" Jxf="0" Glf="0" Lr="0" Zgj="0" />
        <Qdmx Xh="51" Qdbm="050201004001" Mc="地面垫层" Xmtz="100厚碎石垫层，素土夯实" Jsgz="按设计图示尺寸以面积计算，不扣除单个面积0.5m2以内的孔洞" Dw="m2" Sl="295" Zhdj="0" Zhhj="0" Rgf="0" Zcf="0" Fcf="0" Sbf="0" Clf="0" Jxf="0" Glf="0" Lr="0" Zgj="0" />
        <Qdmx Xh="52" Qdbm="050201004002" Mc="地面垫层" Xmtz="150厚C20素砼垫层" Jsgz="按设计图示尺寸以面积计算，不扣除单个面积0.5m2以内的孔洞" Dw="m2" Sl="273" Zhdj="0" Zhhj="0" Rgf="0" Zcf="0" Fcf="0" Sbf="0" Clf="0" Jxf="0" Glf="0" Lr="0" Zgj="0" />
        <Qdmx Xh="53" Qdbm="050201005001" Mc="地面找平层" Xmtz="30厚1:3水泥砂浆内掺防水粉3%" Jsgz="按设计图示尺寸以面积计算，不扣除单个面积0.5m2以内的孔洞" Dw="m2" Sl="273" Zhdj="0" Zhhj="0" Rgf="0" Zcf="0" Fcf="0" Sbf="0" Clf="0" Jxf="0" Glf="0" Lr="0" Zgj="0" />
        <Qdmx Xh="54" Qdbm="050201007001" Mc="橡塑地面面层" Xmtz="13厚EPDM塑胶面层" Jsgz="按设计图示尺寸以面积计算，不扣除单个面积0.5m2以内的孔洞" Dw="m2" Sl="273" Zhdj="0" Zhhj="0" Rgf="0" Zcf="0" Fcf="0" Sbf="0" Clf="0" Jxf="0" Glf="0" Lr="0" Zgj="0" />
        <Qdmx Xh="55" Qdbm="050201006001" Mc="硬质地面面层" Xmtz="150厚C30砼，拉毛防滑处理" Jsgz="按设计图示尺寸以面积计算，不扣除单个面积0.5m2以内的孔洞" Dw="m2" Sl="22" Zhdj="0" Zhhj="0" Rgf="0" Zcf="0" Fcf="0" Sbf="0" Clf="0" Jxf="0" Glf="0" Lr="0" Zgj="0" />
        <Qdmx Xh="56" Qdbm="040305001002" Mc="垫层" Xmtz="坐凳挡墙垫层&#xD;&#xA;100厚碎石垫层，素土夯实" Jsgz="按设计图示尺寸以体积计算" Dw="m3" Sl="3.65" Zhdj="0" Zhhj="0" Rgf="0" Zcf="0" Fcf="0" Sbf="0" Clf="0" Jxf="0" Glf="0" Lr="0" Zgj="0" />
        <Qdmx Xh="57" Qdbm="040305001001" Mc="垫层" Xmtz="坐凳挡墙垫层&#xD;&#xA;150厚C20砼垫层" Jsgz="按设计图示尺寸以体积计算" Dw="m3" Sl="5.47" Zhdj="0" Zhhj="0" Rgf="0" Zcf="0" Fcf="0" Sbf="0" Clf="0" Jxf="0" Glf="0" Lr="0" Zgj="0" />
        <Qdmx Xh="58" Qdbm="010505001002" Mc="垫层模板" Xmtz="垫层木模" Jsgz="按模板与现浇混凝土垫层的接触面积计算" Dw="m2" Sl="11.69" Zhdj="0" Zhhj="0" Rgf="0" Zcf="0" Fcf="0" Sbf="0" Clf="0" Jxf="0" Glf="0" Lr="0" Zgj="0" />
        <Qdmx Xh="59" Qdbm="040305004003" Mc="砖砌体" Xmtz="坐凳挡墙砖砌体&#xD;&#xA;MU10砼砖，M7.5砌筑" Jsgz="按设计图示尺寸以体积计算" Dw="m3" Sl="17.62" Zhdj="0" Zhhj="0" Rgf="0" Zcf="0" Fcf="0" Sbf="0" Clf="0" Jxf="0" Glf="0" Lr="0" Zgj="0" />
        <Qdmx Xh="60" Qdbm="011204001001" Mc="石材零星项目" Xmtz="坐凳挡墙压顶&#xD;&#xA;400*600*30芝麻灰磨光面，含倒角&#xD;&#xA;20厚1:2.5水泥砂浆铺贴" Jsgz="按设计图示镶贴后表面积计算" Dw="m2" Sl="15.2" Zhdj="0" Zhhj="0" Rgf="0" Zcf="0" Fcf="0" Sbf="0" Clf="0" Jxf="0" Glf="0" Lr="0" Zgj="0" />
        <Qdmx Xh="61" Qdbm="011203001001" Mc="石材墙、柱面" Xmtz="坐凳挡墙侧面&#xD;&#xA;400*200*20文化石贴面&#xD;&#xA;20厚1:2.5水泥砂浆" Jsgz="按设计图示镶贴后表面积计算" Dw="m2" Sl="17.1" Zhdj="0" Zhhj="0" Rgf="0" Zcf="0" Fcf="0" Sbf="0" Clf="0" Jxf="0" Glf="0" Lr="0" Zgj="0" />
        <Qdmx Xh="62" Qdbm="050201011002" Mc="路牙" Xmtz="50*200*600水泥侧石，下部砂浆捂牢" Jsgz="按设计图示尺寸以中心线长度计算" Dw="m" Sl="45" Zhdj="0" Zhhj="0" Rgf="0" Zcf="0" Fcf="0" Sbf="0" Clf="0" Jxf="0" Glf="0" Lr="0" Zgj="0" />
        <Qdmx Xh="63" Qdbm="040305001003" Mc="垫层" Xmtz="树池挡墙垫层&#xD;&#xA;100厚碎石垫层，素土夯实" Jsgz="按设计图示尺寸以体积计算" Dw="m3" Sl="0.66" Zhdj="0" Zhhj="0" Rgf="0" Zcf="0" Fcf="0" Sbf="0" Clf="0" Jxf="0" Glf="0" Lr="0" Zgj="0" />
        <Qdmx Xh="64" Qdbm="040305001004" Mc="垫层" Xmtz="树池挡墙垫层&#xD;&#xA;150厚C20砼垫层" Jsgz="按设计图示尺寸以体积计算" Dw="m3" Sl="0.99" Zhdj="0" Zhhj="0" Rgf="0" Zcf="0" Fcf="0" Sbf="0" Clf="0" Jxf="0" Glf="0" Lr="0" Zgj="0" />
        <Qdmx Xh="65" Qdbm="010505001003" Mc="垫层模板" Xmtz="垫层木模" Jsgz="按模板与现浇混凝土垫层的接触面积计算" Dw="m2" Sl="2.07" Zhdj="0" Zhhj="0" Rgf="0" Zcf="0" Fcf="0" Sbf="0" Clf="0" Jxf="0" Glf="0" Lr="0" Zgj="0" />
        <Qdmx Xh="66" Qdbm="040305004004" Mc="砖砌体" Xmtz="树池挡墙砖砌体&#xD;&#xA;MU10砼砖，M7.5砌筑" Jsgz="按设计图示尺寸以体积计算" Dw="m3" Sl="3.2" Zhdj="0" Zhhj="0" Rgf="0" Zcf="0" Fcf="0" Sbf="0" Clf="0" Jxf="0" Glf="0" Lr="0" Zgj="0" />
        <Qdmx Xh="67" Qdbm="011204001002" Mc="石材零星项目" Xmtz="树池挡墙压顶&#xD;&#xA;400*600*30芝麻灰磨光面，弧形定制，含倒角&#xD;&#xA;20厚1:2.5水泥砂浆铺贴" Jsgz="按设计图示镶贴后表面积计算" Dw="m2" Sl="2.76" Zhdj="0" Zhhj="0" Rgf="0" Zcf="0" Fcf="0" Sbf="0" Clf="0" Jxf="0" Glf="0" Lr="0" Zgj="0" />
        <Qdmx Xh="68" Qdbm="011203001002" Mc="石材墙、柱面" Xmtz="树池挡墙侧面&#xD;&#xA;400*200*20文化石贴面&#xD;&#xA;20厚1:2.5水泥砂浆" Jsgz="按设计图示镶贴后表面积计算" Dw="m2" Sl="3.39" Zhdj="0" Zhhj="0" Rgf="0" Zcf="0" Fcf="0" Sbf="0" Clf="0" Jxf="0" Glf="0" Lr="0" Zgj="0" />
        <Qdmx Xh="69" Qdbm="050307020002" Mc="其他景观小摆设" Xmtz="健身器材基础及安装" Jsgz="按设计图示数量计算" Dw="组" Sl="6" Zhdj="0" Zhhj="0" Rgf="0" Zcf="0" Fcf="0" Sbf="0" Clf="0" Jxf="0" Glf="0" Lr="0" Zgj="0" />
      </QdBt>
    </QdBt>
    <QdBt Xh="" Mc="四、绿化清理清杂" Je="0" Zgj="0">
      <Qdmx Xh="70" Qdbm="050101005002" Mc="整理绿化用地" Xmtz="图纸范围内的绿化清理清杂;&#xD;&#xA;对所有民房上的电线及无用废旧支架进行拆除;&#xD;&#xA;对门前屋后的废旧物进行清理;&#xD;&#xA;含废弃物外运及处置费用;" Jsgz="按设计图示尺寸以水平投影面积计算" Dw="项" Sl="1" Zhdj="0" Zhhj="0" Rgf="0" Zcf="0" Fcf="0" Sbf="0" Clf="0" Jxf="0" Glf="0" Lr="0" Zgj="0" />
    </QdBt>
  </Qdxm>
  <Csxm>
    <CsxmBt Xh="" Mc="通用措施项目" Je="0" Bz="">
      <CsxmMx Xh="1" Bm="050406004001" Mc="安全生产" Gznr="" Dw="项" Je="0" Zb_CSSlF="0" Je_CSSlF="0" Zb_ZQYxF="0" Je_ZQYxF="0" Zb_HQCcF="0" Je_HQCcF="0" Qfjs="0" Jsjc="分部分项合计-除税工程设备费" Fl="0.9" Xmlb="1" Jjfs="2" Bz="" />
      <CsxmMx Xh="2" Bm="050406002001" Mc="文明施工" Gznr="" Dw="项" Je="0" Zb_CSSlF="0" Je_CSSlF="0" Zb_ZQYxF="0" Je_ZQYxF="0" Zb_HQCcF="0" Je_HQCcF="0" Qfjs="0" Jsjc="分部分项合计-除税工程设备费" Fl="0" Xmlb="0" Jjfs="2" Bz="" />
      <CsxmMx Xh="3" Bm="050406003001" Mc="环境保护" Gznr="" Dw="项" Je="0" Zb_CSSlF="0" Je_CSSlF="0" Zb_ZQYxF="0" Je_ZQYxF="0" Zb_HQCcF="0" Je_HQCcF="0" Qfjs="0" Jsjc="分部分项合计-除税工程设备费" Fl="0" Xmlb="0" Jjfs="2" Bz="" />
      <CsxmMx Xh="4" Bm="050406001001" Mc="临时设施" Gznr="" Dw="项" Je="0" Zb_CSSlF="0" Je_CSSlF="0" Zb_ZQYxF="0" Je_ZQYxF="0" Zb_HQCcF="0" Je_HQCcF="0" Qfjs="0" Jsjc="分部分项合计-除税工程设备费" Fl="0" Xmlb="0" Jjfs="2" Bz="" />
      <CsxmMx Xh="5" Bm="050406005001" Mc="冬雨季施工" Gznr="" Dw="项" Je="0" Zb_CSSlF="0" Je_CSSlF="0" Zb_ZQYxF="0" Je_ZQYxF="0" Zb_HQCcF="0" Je_HQCcF="0" Qfjs="0" Jsjc="分部分项合计-除税工程设备费" Fl="0" Xmlb="0" Jjfs="2" Bz="" />
      <CsxmMx Xh="6" Bm="050406006001" Mc="夜间施工" Gznr="" Dw="项" Je="0" Zb_CSSlF="0" Je_CSSlF="0" Zb_ZQYxF="0" Je_ZQYxF="0" Zb_HQCcF="0" Je_HQCcF="0" Qfjs="0" Jsjc="分部分项合计-除税工程设备费" Fl="0" Xmlb="0" Jjfs="2" Bz="" />
      <CsxmMx Xh="7" Bm="050406007001" Mc="特殊地区施工增加" Gznr="" Dw="项" Je="0" Zb_CSSlF="0" Je_CSSlF="0" Zb_ZQYxF="0" Je_ZQYxF="0" Zb_HQCcF="0" Je_HQCcF="0" Qfjs="0" Jsjc="分部分项合计-除税工程设备费" Fl="0" Xmlb="0" Jjfs="2" Bz="" />
      <CsxmMx Xh="8" Bm="050406008001" Mc="二次搬运" Gznr="" Dw="项" Je="0" Zb_CSSlF="0" Je_CSSlF="0" Zb_ZQYxF="0" Je_ZQYxF="0" Zb_HQCcF="0" Je_HQCcF="0" Qfjs="0" Jsjc="分部分项合计-除税工程设备费" Fl="0" Xmlb="0" Jjfs="2" Bz="" />
      <CsxmMx Xh="9" Bm="050406009001" Mc="已完工程及设备保护" Gznr="" Dw="项" Je="0" Zb_CSSlF="0" Je_CSSlF="0" Zb_ZQYxF="0" Je_ZQYxF="0" Zb_HQCcF="0" Je_HQCcF="0" Qfjs="0" Jsjc="分部分项合计-除税工程设备费" Fl="0" Xmlb="0" Jjfs="2" Bz="" />
      <CsxmMx Xh="10" Bm="050406010001" Mc="既有建(构)筑物、设施保护" Gznr="" Dw="项" Je="0" Zb_CSSlF="0" Je_CSSlF="0" Zb_ZQYxF="0" Je_ZQYxF="0" Zb_HQCcF="0" Je_HQCcF="0" Qfjs="0" Jsjc="分部分项合计-除税工程设备费" Fl="0" Xmlb="0" Jjfs="2" Bz="" />
      <CsxmMx Xh="11" Bm="050406011001" Mc="按质论价" Gznr="" Dw="项" Je="0" Zb_CSSlF="0" Je_CSSlF="0" Zb_ZQYxF="0" Je_ZQYxF="0" Zb_HQCcF="0" Je_HQCcF="0" Qfjs="0" Jsjc="分部分项合计-除税工程设备费" Fl="0" Xmlb="2" Jjfs="2" Bz="" />
      <CsxmMx Xh="12" Bm="050406012001" Mc="建筑工人实名制" Gznr="" Dw="项" Je="0" Zb_CSSlF="0" Je_CSSlF="0" Zb_ZQYxF="0" Je_ZQYxF="0" Zb_HQCcF="0" Je_HQCcF="0" Qfjs="0" Jsjc="分部分项合计-除税工程设备费" Fl="0" Xmlb="0" Jjfs="2" Bz="" />
      <CsxmMx Xh="13" Bm="050406013001" Mc="特殊施工降效" Gznr="" Dw="项" Je="0" Zb_CSSlF="0" Je_CSSlF="0" Zb_ZQYxF="0" Je_ZQYxF="0" Zb_HQCcF="0" Je_HQCcF="0" Qfjs="0" Jsjc="分部分项合计-除税工程设备费" Fl="0" Xmlb="0" Jjfs="2" Bz="" />
      <CsxmMx Xh="14" Bm="050406014001" Mc="协管" Gznr="" Dw="项" Je="0" Zb_CSSlF="0" Je_CSSlF="0" Zb_ZQYxF="0" Je_ZQYxF="0" Zb_HQCcF="0" Je_HQCcF="0" Qfjs="0" Jsjc="分部分项合计-除税工程设备费" Fl="0" Xmlb="0" Jjfs="2" Bz="" />
    </CsxmBt>
    <CsxmBt Xh="" Mc="专业措施项目" Je="0" Bz="">
      <CsxmMx Xh="15" Bm="050404002001" Mc="大型机械设备进出场及安拆" Gznr="" Dw="项" Je="0" Zb_CSSlF="0" Je_CSSlF="0" Zb_ZQYxF="0" Je_ZQYxF="0" Zb_HQCcF="0" Je_HQCcF="0" Xmlb="3" Jjfs="1" Bz="" />
      <CsxmMx Xh="16" Bm="050405002001" Mc="排水" Gznr="原有水塘排水" Dw="项" Je="0" Zb_CSSlF="0" Je_CSSlF="0" Zb_ZQYxF="0" Je_ZQYxF="0" Zb_HQCcF="0" Je_HQCcF="0" Xmlb="0" Jjfs="1" Bz="" />
    </CsxmBt>
  </Csxm>
  <Qtxm>
    <QtxmMx Xh="1" Mc="暂列金额" Je="0" Bz="详见本标准表E.4.2" Xmlb="1" />
    <QtxmMx Xh="2" Mc="专业工程暂估价" Je="0" Bz="详见本标准表E.4.3" Xmlb="2" />
    <QtxmMx Xh="3" Mc="计日工" Je="0" Bz="详见本标准表E.4.4" Xmlb="3" />
    <QtxmMx Xh="4" Mc="总承包服务费" Je="0" Bz="详见本标准表E.4.5" Xmlb="4" />
    <QtxmMx Xh="5" Mc="合同中约定的其他项目" Je="0" Bz="" Xmlb="5" />
  </Qtxm>
  <Zlje>
    <ZljeBt Xh="1" Mc="合同价格调整暂列金额" Je="0" Xmlb="1" />
    <ZljeBt Xh="2" Mc="未确定工程暂列金额" Je="0" Xmlb="2" />
    <ZljeBt Xh="3" Mc="未确定服务暂列金额" Je="0" Xmlb="3" />
    <ZljeBt Xh="4" Mc="未确定其他暂列金额" Je="0" Xmlb="4" />
  </Zlje>
  <Zygczgj />
  <Jrg>
    <JrgBt Bh="一" Mc="人工" Je="0" Xmlb="1" />
    <JrgBt Bh="二" Mc="材料" Je="0" Xmlb="2" />
    <JrgBt Bh="三" Mc="施工机具" Je="0" Xmlb="3" />
  </Jrg>
  <Zcbfwf>
    <ZcbfwfBt Xh="1" Mc="发包人提供材料" Je="0" Xmlb="1" />
    <ZcbfwfBt Xh="2" Mc="专业分包工程" Je="0" Xmlb="2" />
    <ZcbfwfBt Xh="3" Mc="直接发包的专业工程" Je="0" Xmlb="3" />
  </Zcbfwf>
  <Clzg />
  <Fbrgycl />
  <CbrgyclCef />
  <Rcjhz />
</Dwgcxx>
  </Dxgcxx>
</JingJiBiao>